#MicroXplorer Configuration settings - do not modify
CAD.formats=
CAD.pinconfig=
CAD.provider=
ETH.IPParameters=MediaInterface,PhyAddress,MACAddr
ETH.MACAddr=00\:80\:E1\:00\:00\:44
ETH.MediaInterface=HAL_ETH_RMII_MODE
ETH.PhyAddress=0
File.Version=6
KeepUserPlacement=true
LTDC.ActiveH=272
LTDC.ActiveW=480
LTDC.Alpha_L0=255
LTDC.Alpha_L1=255
LTDC.BlendingFactor1_L0=LTDC_BLENDING_FACTOR1_PAxCA
LTDC.BlendingFactor1_L1=LTDC_BLENDING_FACTOR1_PAxCA
LTDC.BlendingFactor2_L0=LTDC_BLENDING_FACTOR2_PAxCA
LTDC.BlendingFactor2_L1=LTDC_BLENDING_FACTOR2_PAxCA
LTDC.Green=255
LTDC.HBP=13
LTDC.HFP=32
LTDC.HSync=41
LTDC.IPParameters=WindowX1_L0,WindowY1_L0,WindowX1_L1,WindowY1_L1,Alpha_L0,BlendingFactor1_L0,BlendingFactor2_L0,Alpha_L1,ImageWidth_L0,ImageHeight_L0,ImageWidth_L1,ImageHeight_L1,PixelFormat_L0,PixelFormat_L1,HSync,HBP,ActiveW,HFP,VSync,ActiveH,Green,BlendingFactor1_L1,BlendingFactor2_L1
LTDC.ImageHeight_L0=272
LTDC.ImageHeight_L1=272
LTDC.ImageWidth_L0=480
LTDC.ImageWidth_L1=480
LTDC.PixelFormat_L0=LTDC_PIXEL_FORMAT_ARGB1555
LTDC.PixelFormat_L1=LTDC_PIXEL_FORMAT_ARGB1555
LTDC.VSync=10
LTDC.WindowX1_L0=480
LTDC.WindowX1_L1=480
LTDC.WindowY1_L0=272
LTDC.WindowY1_L1=272
LWIP.BSP.number=1
LWIP.IPParameters=LWIP_DHCP,IP_ADDRESS,NETMASK_ADDRESS,LWIP_HTTPD,LWIP_HTTPD_CUSTOM_FILES,LWIP_HTTPD_CGI_SSI,LWIP_HTTPD_SSI,LWIP_HTTPD_SSI_RAW,LWIP_DNS,MEMP_MEM_MALLOC,LWIP_IGMP,LWIP_HTTPD_CGI,LWIP_HTTPD_SUPPORT_POST,MEM_LIBC_MALLOC,LWIP_TFTP
LWIP.IP_ADDRESS=192.168.069.010
LWIP.LWIP_DHCP=0
LWIP.LWIP_DNS=1
LWIP.LWIP_HTTPD=1
LWIP.LWIP_HTTPD_CGI=1
LWIP.LWIP_HTTPD_CGI_SSI=1
LWIP.LWIP_HTTPD_CUSTOM_FILES=1
LWIP.LWIP_HTTPD_SSI=1
LWIP.LWIP_HTTPD_SSI_RAW=1
LWIP.LWIP_HTTPD_SUPPORT_POST=1
LWIP.LWIP_IGMP=1
LWIP.LWIP_TFTP=1
LWIP.MEMP_MEM_MALLOC=1
LWIP.MEM_LIBC_MALLOC=1
LWIP.NETMASK_ADDRESS=255.255.255.000
LWIP.Version=v2.1.2_Cube
LWIP0.BSP.STBoard=false
LWIP0.BSP.api=BSP_COMPONENT_DRIVER
LWIP0.BSP.component=LAN8742
LWIP0.BSP.condition=
LWIP0.BSP.instance=LAN8742
LWIP0.BSP.ip=
LWIP0.BSP.mode=
LWIP0.BSP.name=Driver_PHY
LWIP0.BSP.semaphore=S_LAN8742
LWIP0.BSP.solution=LAN8742
Mcu.CPN=STM32F746NGH6
Mcu.Family=STM32F7
Mcu.IP0=CORTEX_M7
Mcu.IP1=DMA2D
Mcu.IP10=USART1
Mcu.IP2=ETH
Mcu.IP3=FMC
Mcu.IP4=LTDC
Mcu.IP5=LWIP
Mcu.IP6=NVIC
Mcu.IP7=QUADSPI
Mcu.IP8=RCC
Mcu.IP9=SYS
Mcu.IPNb=11
Mcu.Name=STM32F746NGHx
Mcu.Package=TFBGA216
Mcu.Pin0=PE4
Mcu.Pin1=PE2
Mcu.Pin10=PJ13
Mcu.Pin11=PD0
Mcu.Pin12=PK7
Mcu.Pin13=PK6
Mcu.Pin14=PK5
Mcu.Pin15=PG12
Mcu.Pin16=PJ14
Mcu.Pin17=PD1
Mcu.Pin18=PF0
Mcu.Pin19=PI10
Mcu.Pin2=PG14
Mcu.Pin20=PK4
Mcu.Pin21=PK3
Mcu.Pin22=PJ15
Mcu.Pin23=PI1
Mcu.Pin24=PC14/OSC32_IN
Mcu.Pin25=PF1
Mcu.Pin26=PI12
Mcu.Pin27=PI9
Mcu.Pin28=PA9
Mcu.Pin29=PC15/OSC32_OUT
Mcu.Pin3=PE1
Mcu.Pin30=PI11
Mcu.Pin31=PK1
Mcu.Pin32=PK2
Mcu.Pin33=PH0/OSC_IN
Mcu.Pin34=PF2
Mcu.Pin35=PI15
Mcu.Pin36=PJ11
Mcu.Pin37=PK0
Mcu.Pin38=PH1/OSC_OUT
Mcu.Pin39=PF3
Mcu.Pin4=PE0
Mcu.Pin40=PI14
Mcu.Pin41=PJ8
Mcu.Pin42=PJ10
Mcu.Pin43=PG8
Mcu.Pin44=PF4
Mcu.Pin45=PH5
Mcu.Pin46=PH3
Mcu.Pin47=PJ7
Mcu.Pin48=PJ9
Mcu.Pin49=PF5
Mcu.Pin5=PG13
Mcu.Pin50=PH2
Mcu.Pin51=PJ6
Mcu.Pin52=PD15
Mcu.Pin53=PD10
Mcu.Pin54=PD14
Mcu.Pin55=PD9
Mcu.Pin56=PD8
Mcu.Pin57=PC1
Mcu.Pin58=PB2
Mcu.Pin59=PF12
Mcu.Pin6=PB7
Mcu.Pin60=PG1
Mcu.Pin61=PF15
Mcu.Pin62=PJ4
Mcu.Pin63=PD12
Mcu.Pin64=PD13
Mcu.Pin65=PJ5
Mcu.Pin66=PA1
Mcu.Pin67=PC4
Mcu.Pin68=PF13
Mcu.Pin69=PG0
Mcu.Pin7=PB6
Mcu.Pin70=PJ3
Mcu.Pin71=PE8
Mcu.Pin72=PD11
Mcu.Pin73=PG5
Mcu.Pin74=PG4
Mcu.Pin75=PA2
Mcu.Pin76=PC5
Mcu.Pin77=PF14
Mcu.Pin78=PJ2
Mcu.Pin79=PF11
Mcu.Pin8=PG15
Mcu.Pin80=PE9
Mcu.Pin81=PE11
Mcu.Pin82=PE14
Mcu.Pin83=PA7
Mcu.Pin84=PJ0
Mcu.Pin85=PJ1
Mcu.Pin86=PE7
Mcu.Pin87=PE10
Mcu.Pin88=PE12
Mcu.Pin89=PE15
Mcu.Pin9=PG11
Mcu.Pin90=PE13
Mcu.Pin91=VP_DMA2D_VS_DMA2D
Mcu.Pin92=VP_LWIP_VS_Enabled
Mcu.Pin93=VP_SYS_VS_Systick
Mcu.PinsNb=94
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32F746NGHx
MxCube.Version=6.8.1
MxDb.Version=DB.6.0.81
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:false\:true\:false\:false
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:false\:true\:false\:false
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:false\:true\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:false\:true\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:false\:true\:false\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:true\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:true\:true\:false\:false
NVIC.SysTick_IRQn=true\:0\:0\:false\:false\:true\:true\:true\:false
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:false\:true\:false\:false
PA1.Mode=RMII
PA1.Signal=ETH_REF_CLK
PA2.Mode=RMII
PA2.Signal=ETH_MDIO
PA7.Mode=RMII
PA7.Signal=ETH_CRS_DV
PA9.Locked=true
PA9.Mode=Asynchronous
PA9.Signal=USART1_TX
PB2.Mode=Single Bank 1
PB2.Signal=QUADSPI_CLK
PB6.Mode=Single Bank 1
PB6.Signal=QUADSPI_BK1_NCS
PB7.Mode=Asynchronous
PB7.Signal=USART1_RX
PC1.Mode=RMII
PC1.Signal=ETH_MDC
PC14/OSC32_IN.Mode=LSE-External-Oscillator
PC14/OSC32_IN.Signal=RCC_OSC32_IN
PC15/OSC32_OUT.Mode=LSE-External-Oscillator
PC15/OSC32_OUT.Signal=RCC_OSC32_OUT
PC4.Mode=RMII
PC4.Signal=ETH_RXD0
PC5.Mode=RMII
PC5.Signal=ETH_RXD1
PD0.Signal=FMC_D2_DA2
PD1.Signal=FMC_D3_DA3
PD10.Signal=FMC_D15_DA15
PD11.Locked=true
PD11.Mode=Single Bank 1
PD11.Signal=QUADSPI_BK1_IO0
PD12.Locked=true
PD12.Mode=Single Bank 1
PD12.Signal=QUADSPI_BK1_IO1
PD13.Locked=true
PD13.Mode=Single Bank 1
PD13.Signal=QUADSPI_BK1_IO3
PD14.Signal=FMC_D0_DA0
PD15.Signal=FMC_D1_DA1
PD8.Signal=FMC_D13_DA13
PD9.Signal=FMC_D14_DA14
PE0.Signal=FMC_NBL0
PE1.Signal=FMC_NBL1
PE10.Signal=FMC_D7_DA7
PE11.Signal=FMC_D8_DA8
PE12.Signal=FMC_D9_DA9
PE13.Signal=FMC_D10_DA10
PE14.Signal=FMC_D11_DA11
PE15.Signal=FMC_D12_DA12
PE2.Mode=Single Bank 1
PE2.Signal=QUADSPI_BK1_IO2
PE4.Mode=RGB888
PE4.Signal=LTDC_B0
PE7.Signal=FMC_D4_DA4
PE8.Signal=FMC_D5_DA5
PE9.Signal=FMC_D6_DA6
PF0.Signal=FMC_A0
PF1.Signal=FMC_A1
PF11.Signal=FMC_SDNRAS
PF12.Signal=FMC_A6
PF13.Signal=FMC_A7
PF14.Signal=FMC_A8
PF15.Signal=FMC_A9
PF2.Signal=FMC_A2
PF3.Signal=FMC_A3
PF4.Signal=FMC_A4
PF5.Signal=FMC_A5
PG0.Signal=FMC_A10
PG1.Signal=FMC_A11
PG11.Mode=RMII
PG11.Signal=ETH_TX_EN
PG12.Locked=true
PG12.Mode=RGB888
PG12.Signal=LTDC_B4
PG13.Mode=RMII
PG13.Signal=ETH_TXD0
PG14.Mode=RMII
PG14.Signal=ETH_TXD1
PG15.Signal=FMC_SDNCAS
PG4.Signal=FMC_A14_BA0
PG5.Signal=FMC_A15_BA1
PG8.Signal=FMC_SDCLK
PH0/OSC_IN.Mode=HSE-External-Oscillator
PH0/OSC_IN.Signal=RCC_OSC_IN
PH1/OSC_OUT.Mode=HSE-External-Oscillator
PH1/OSC_OUT.Signal=RCC_OSC_OUT
PH2.Mode=SdramChipSelect1_1
PH2.Signal=FMC_SDCKE0
PH3.Mode=SdramChipSelect1_1
PH3.Signal=FMC_SDNE0
PH5.Signal=FMC_SDNWE
PI1.GPIOParameters=GPIO_Label
PI1.GPIO_Label=LED
PI1.Locked=true
PI1.Signal=GPIO_Output
PI10.Mode=RGB888
PI10.Signal=LTDC_HSYNC
PI11.GPIOParameters=GPIO_Label
PI11.GPIO_Label=BUTTON
PI11.Locked=true
PI11.Signal=GPIO_Input
PI12.GPIOParameters=GPIO_Label
PI12.GPIO_Label=LCD_DISP
PI12.Locked=true
PI12.Signal=GPIO_Output
PI14.Mode=RGB888
PI14.Signal=LTDC_CLK
PI15.Locked=true
PI15.Mode=RGB888
PI15.Signal=LTDC_R0
PI9.Mode=RGB888
PI9.Signal=LTDC_VSYNC
PJ0.Locked=true
PJ0.Mode=RGB888
PJ0.Signal=LTDC_R1
PJ1.Locked=true
PJ1.Mode=RGB888
PJ1.Signal=LTDC_R2
PJ10.Locked=true
PJ10.Mode=RGB888
PJ10.Signal=LTDC_G3
PJ11.Locked=true
PJ11.Mode=RGB888
PJ11.Signal=LTDC_G4
PJ13.Mode=RGB888
PJ13.Signal=LTDC_B1
PJ14.Locked=true
PJ14.Mode=RGB888
PJ14.Signal=LTDC_B2
PJ15.Locked=true
PJ15.Mode=RGB888
PJ15.Signal=LTDC_B3
PJ2.Locked=true
PJ2.Mode=RGB888
PJ2.Signal=LTDC_R3
PJ3.Locked=true
PJ3.Mode=RGB888
PJ3.Signal=LTDC_R4
PJ4.Locked=true
PJ4.Mode=RGB888
PJ4.Signal=LTDC_R5
PJ5.Locked=true
PJ5.Mode=RGB888
PJ5.Signal=LTDC_R6
PJ6.Locked=true
PJ6.Mode=RGB888
PJ6.Signal=LTDC_R7
PJ7.Locked=true
PJ7.Mode=RGB888
PJ7.Signal=LTDC_G0
PJ8.Locked=true
PJ8.Mode=RGB888
PJ8.Signal=LTDC_G1
PJ9.Locked=true
PJ9.Mode=RGB888
PJ9.Signal=LTDC_G2
PK0.Locked=true
PK0.Mode=RGB888
PK0.Signal=LTDC_G5
PK1.Locked=true
PK1.Mode=RGB888
PK1.Signal=LTDC_G6
PK2.Locked=true
PK2.Mode=RGB888
PK2.Signal=LTDC_G7
PK3.GPIOParameters=GPIO_Label
PK3.GPIO_Label=LCD_BL_CTRL
PK3.Locked=true
PK3.Signal=GPIO_Output
PK4.Locked=true
PK4.Mode=RGB888
PK4.Signal=LTDC_B5
PK5.Locked=true
PK5.Mode=RGB888
PK5.Signal=LTDC_B6
PK6.Locked=true
PK6.Mode=RGB888
PK6.Signal=LTDC_B7
PK7.Mode=RGB888
PK7.Signal=LTDC_DE
PinOutPanel.CurrentBGAView=Top
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32F746NGHx
ProjectManager.FirmwarePackage=STM32Cube FW_F7 V1.17.1
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=STM32CubeIDE
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=project.ioc
ProjectManager.ProjectName=project
ProjectManager.ProjectStructure=
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-HAL-true,2-SystemClock_Config-RCC-false-HAL-true,3-MX_LTDC_Init-LTDC-false-HAL-true,4-MX_USART1_UART_Init-USART1-false-HAL-true,5-MX_DMA2D_Init-DMA2D-false-HAL-true,6-MX_FMC_Init-FMC-false-HAL-true,7-MX_LWIP_Init-LWIP-false-HAL-false,8-MX_QUADSPI_Init-QUADSPI-false-HAL-true,0-MX_CORTEX_M7_Init-CORTEX_M7-false-HAL-true
QUADSPI.ChipSelectHighTime=QSPI_CS_HIGH_TIME_6_CYCLE
QUADSPI.ClockPrescaler=1
QUADSPI.FifoThreshold=4
QUADSPI.FlashSize=16
QUADSPI.IPParameters=ClockPrescaler,FifoThreshold,SampleShifting,FlashSize,ChipSelectHighTime
QUADSPI.SampleShifting=QSPI_SAMPLE_SHIFTING_HALFCYCLE
RCC.AHBFreq_Value=200000000
RCC.APB1CLKDivider=RCC_HCLK_DIV4
RCC.APB1Freq_Value=50000000
RCC.APB1TimFreq_Value=100000000
RCC.APB2CLKDivider=RCC_HCLK_DIV2
RCC.APB2Freq_Value=100000000
RCC.APB2TimFreq_Value=200000000
RCC.CECFreq_Value=32786.88524590164
RCC.CortexFreq_Value=200000000
RCC.EthernetFreq_Value=200000000
RCC.FCLKCortexFreq_Value=200000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=200000000
RCC.HSE_VALUE=25000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=50000000
RCC.I2C2Freq_Value=50000000
RCC.I2C3Freq_Value=50000000
RCC.I2C4Freq_Value=50000000
RCC.I2SFreq_Value=96000000
RCC.IPParameters=AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2CLKDivider,APB2Freq_Value,APB2TimFreq_Value,CECFreq_Value,CortexFreq_Value,EthernetFreq_Value,FCLKCortexFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2C4Freq_Value,I2SFreq_Value,LCDTFToutputFreq_Value,LPTIM1Freq_Value,LSI_VALUE,MCO2PinFreq_Value,PLLCLKFreq_Value,PLLI2SPCLKFreq_Value,PLLI2SQCLKFreq_Value,PLLI2SRCLKFreq_Value,PLLI2SRoutputFreq_Value,PLLM,PLLN,PLLQCLKFreq_Value,PLLQoutputFreq_Value,PLLSAIPCLKFreq_Value,PLLSAIQCLKFreq_Value,PLLSAIR,PLLSAIRCLKFreq_Value,PLLSAIRDiv,PLLSAIoutputFreq_Value,PLLSourceVirtual,RNGFreq_Value,SAI1Freq_Value,SAI2Freq_Value,SDMMCFreq_Value,SPDIFRXFreq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,UART5Freq_Value,UART7Freq_Value,UART8Freq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USART6Freq_Value,USBFreq_Value,VCOI2SOutputFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOSAIOutputFreq_Value
RCC.LCDTFToutputFreq_Value=9600000
RCC.LPTIM1Freq_Value=50000000
RCC.LSI_VALUE=32000
RCC.MCO2PinFreq_Value=200000000
RCC.PLLCLKFreq_Value=200000000
RCC.PLLI2SPCLKFreq_Value=96000000
RCC.PLLI2SQCLKFreq_Value=96000000
RCC.PLLI2SRCLKFreq_Value=96000000
RCC.PLLI2SRoutputFreq_Value=96000000
RCC.PLLM=25
RCC.PLLN=400
RCC.PLLQCLKFreq_Value=200000000
RCC.PLLQoutputFreq_Value=200000000
RCC.PLLSAIPCLKFreq_Value=96000000
RCC.PLLSAIQCLKFreq_Value=96000000
RCC.PLLSAIR=5
RCC.PLLSAIRCLKFreq_Value=38400000
RCC.PLLSAIRDiv=RCC_PLLSAIDIVR_4
RCC.PLLSAIoutputFreq_Value=96000000
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.RNGFreq_Value=200000000
RCC.SAI1Freq_Value=96000000
RCC.SAI2Freq_Value=96000000
RCC.SDMMCFreq_Value=200000000
RCC.SPDIFRXFreq_Value=96000000
RCC.SYSCLKFreq_VALUE=200000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=50000000
RCC.UART5Freq_Value=50000000
RCC.UART7Freq_Value=50000000
RCC.UART8Freq_Value=50000000
RCC.USART1Freq_Value=100000000
RCC.USART2Freq_Value=50000000
RCC.USART3Freq_Value=50000000
RCC.USART6Freq_Value=100000000
RCC.USBFreq_Value=200000000
RCC.VCOI2SOutputFreq_Value=192000000
RCC.VCOInputFreq_Value=1000000
RCC.VCOOutputFreq_Value=400000000
RCC.VCOSAIOutputFreq_Value=192000000
SH.FMC_A0.0=FMC_A0,12b-sda1
SH.FMC_A0.ConfNb=1
SH.FMC_A1.0=FMC_A1,12b-sda1
SH.FMC_A1.ConfNb=1
SH.FMC_A10.0=FMC_A10,12b-sda1
SH.FMC_A10.ConfNb=1
SH.FMC_A11.0=FMC_A11,12b-sda1
SH.FMC_A11.ConfNb=1
SH.FMC_A14_BA0.0=FMC_BA0,FourSdramBanks1
SH.FMC_A14_BA0.ConfNb=1
SH.FMC_A15_BA1.0=FMC_BA1,FourSdramBanks1
SH.FMC_A15_BA1.ConfNb=1
SH.FMC_A2.0=FMC_A2,12b-sda1
SH.FMC_A2.ConfNb=1
SH.FMC_A3.0=FMC_A3,12b-sda1
SH.FMC_A3.ConfNb=1
SH.FMC_A4.0=FMC_A4,12b-sda1
SH.FMC_A4.ConfNb=1
SH.FMC_A5.0=FMC_A5,12b-sda1
SH.FMC_A5.ConfNb=1
SH.FMC_A6.0=FMC_A6,12b-sda1
SH.FMC_A6.ConfNb=1
SH.FMC_A7.0=FMC_A7,12b-sda1
SH.FMC_A7.ConfNb=1
SH.FMC_A8.0=FMC_A8,12b-sda1
SH.FMC_A8.ConfNb=1
SH.FMC_A9.0=FMC_A9,12b-sda1
SH.FMC_A9.ConfNb=1
SH.FMC_D0_DA0.0=FMC_D0,sd-16b-d1
SH.FMC_D0_DA0.ConfNb=1
SH.FMC_D10_DA10.0=FMC_D10,sd-16b-d1
SH.FMC_D10_DA10.ConfNb=1
SH.FMC_D11_DA11.0=FMC_D11,sd-16b-d1
SH.FMC_D11_DA11.ConfNb=1
SH.FMC_D12_DA12.0=FMC_D12,sd-16b-d1
SH.FMC_D12_DA12.ConfNb=1
SH.FMC_D13_DA13.0=FMC_D13,sd-16b-d1
SH.FMC_D13_DA13.ConfNb=1
SH.FMC_D14_DA14.0=FMC_D14,sd-16b-d1
SH.FMC_D14_DA14.ConfNb=1
SH.FMC_D15_DA15.0=FMC_D15,sd-16b-d1
SH.FMC_D15_DA15.ConfNb=1
SH.FMC_D1_DA1.0=FMC_D1,sd-16b-d1
SH.FMC_D1_DA1.ConfNb=1
SH.FMC_D2_DA2.0=FMC_D2,sd-16b-d1
SH.FMC_D2_DA2.ConfNb=1
SH.FMC_D3_DA3.0=FMC_D3,sd-16b-d1
SH.FMC_D3_DA3.ConfNb=1
SH.FMC_D4_DA4.0=FMC_D4,sd-16b-d1
SH.FMC_D4_DA4.ConfNb=1
SH.FMC_D5_DA5.0=FMC_D5,sd-16b-d1
SH.FMC_D5_DA5.ConfNb=1
SH.FMC_D6_DA6.0=FMC_D6,sd-16b-d1
SH.FMC_D6_DA6.ConfNb=1
SH.FMC_D7_DA7.0=FMC_D7,sd-16b-d1
SH.FMC_D7_DA7.ConfNb=1
SH.FMC_D8_DA8.0=FMC_D8,sd-16b-d1
SH.FMC_D8_DA8.ConfNb=1
SH.FMC_D9_DA9.0=FMC_D9,sd-16b-d1
SH.FMC_D9_DA9.ConfNb=1
SH.FMC_NBL0.0=FMC_NBL0,Sd2ByteEnable1
SH.FMC_NBL0.ConfNb=1
SH.FMC_NBL1.0=FMC_NBL1,Sd2ByteEnable1
SH.FMC_NBL1.ConfNb=1
SH.FMC_SDCLK.0=FMC_SDCLK,12b-sda1
SH.FMC_SDCLK.ConfNb=1
SH.FMC_SDNCAS.0=FMC_SDNCAS,12b-sda1
SH.FMC_SDNCAS.ConfNb=1
SH.FMC_SDNRAS.0=FMC_SDNRAS,12b-sda1
SH.FMC_SDNRAS.ConfNb=1
SH.FMC_SDNWE.0=FMC_SDNWE,12b-sda1
SH.FMC_SDNWE.ConfNb=1
USART1.IPParameters=WordLength,VirtualMode,VirtualMode-Asynchronous
USART1.VirtualMode=VM_ASYNC
USART1.VirtualMode-Asynchronous=VM_ASYNC
USART1.WordLength=WORDLENGTH_8B
VP_DMA2D_VS_DMA2D.Mode=DMA2D_Activate
VP_DMA2D_VS_DMA2D.Signal=DMA2D_VS_DMA2D
VP_LWIP_VS_Enabled.Mode=Enabled
VP_LWIP_VS_Enabled.Signal=LWIP_VS_Enabled
VP_SYS_VS_Systick.Mode=SysTick
VP_SYS_VS_Systick.Signal=SYS_VS_Systick
board=STM32F746G-DISCO
boardIOC=true
isbadioc=false
